For 1990-2009 cars

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 43184 Valve Spring Compressor Adaptor

• | J 36017 Valve Guide Seal Remover

Caution: Wear safety glasses in order to avoid eye damage.

Important: Ensure that the valve train components are kept together and identified in order for proper re-installation in their original position.

1. Compress the valve spring. Use the J 8062 .
2. Remove the valve keepers. Use the J 43184 (2).
3. Slowly release the J 8062 from the valve spring assembly.
4. Remove the retainer (4).
5. Remove the spring (3).
6. Remove the spring seats (2).

Notice: Do not damage the valve guide. Remove any burrs that have formed at the key groove by chamfering the valve stem with an oil stone or a file.

7. Remove the valve seal.
8. Remove the valve.
9. Remove the remaining valve springs and valves.