For 1990-2009 cars

### Removal Procedure

1. Remove the following from the check valve:

• | The hose clamp

• | The hose

2. Remove the valve from the tube.
3. Remove the following from the booster assembly (1):

• | The hose clamp

• | The hose

• | The check valve

### Installation Procedure

1. Install the hose to the booster assembly (1). Secure with the hose clamp.
2. Install the valve to the tube.
3. Install the hose to the check valve. Secure with the hose clamp.