For 1990-2009 cars

### Removal Procedure

1. Remove the left body hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement in Interior Trim.
2. Remove the 2 bolts (3) which secure the IP drivers knee bolster trim (1). Position the trim as necessary to gain access to the IP drivers knee bolster reinforcement.
3. Remove the following components from the vehicle:

• | The 2 bolts which secure the reinforcement

• | The IP drivers knee bolster reinforcement (1)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the IP drivers knee bolster reinforcement (1) to the instrument panel. Secure the reinforcement with the 2 bolts.

Tighten
Tighten the knee bolster reinforcement bolts to 10 N·m (89 lb in).

2. Install the IP drivers knee bolster trim (1) to the instrument panel assembly. Secure the trim with the 2 bolts (3).

Tighten
Tighten the knee bolster trim bolts to 10 N·m (89 lb in).

3. Install the left body hinge pillar trim panel. Refer to Body Hinge Pillar Trim Panel Replacement in Interior Trim.