For 1990-2009 cars

### Removal Procedure

1. Disengage the front retaining clips (2) by raising the rear seat cushion (1) at the front edge.
2. Pull the rear seat cushion (1) forward in order to remove the cushion from the vehicle.

### Installation Procedure

1. Slide the rear seat cushion (1) into position. Ensure that the seat belt buckles are properly position through the cushion.
2. Engage the rear seat cushion front retaining clips (2).