For 1990-2009 cars

### Removal Procedure

1. Push in the tab (2) on the head restraint guides.
2. Lift and remove the head restraint (1).
3. Release the tab on the side of the head restraint guide. Remove the guides (1) from the seat back cushion (2) by gently prying with a flat bladed tool, if necessary.

### Installation Procedure

1. Install the head restraint guides to the seat back cushion, if removed.
2. Push in the tabs (2) on the head restraint guides.
3. Install the head restraint (1).