For 1990-2009 cars

### Circuit Description

This DTC allows the cruise control module to check for unwanted application of the servo due to a malfunction within the cruise control module.

### Diagnostic Aids

Check for a faulty cruise control module.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Cruise Control Diagnostic System Check performed? | -- | Go to Step 2 | Go to Cruise Control System Check
2 |

1. Turn the ignition switch to the LOCK position.
2. Clear any DTCs present.
3. Test drive the vehicle at approximately 80 km/h (50 mph).
4. Engage the cruise control and observe the performance for one minute.
5. Stop the vehicle and test for DTCs.

Does this DTC reset?

--

Go to Step 3

Go to Step 4

3 | Replace the cruise control module. Is the repair complete? | -- | Go to Cruise Control System Check | --
4 | Malfunction is not present at this time. Refer to diagnostic aids for additional information. Is the action complete? | -- | Go to Cruise Control System Check | --