For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia (6). Refer to Rear Bumper Fascia Replacement .
2. Remove the rear bumper fascia energy absorber (4) from the rear bumper impact bar (2).

### Installation Procedure

1. Install the rear bumper fascia energy absorber (4) to the rear bumper impact bar (2).
2. Install the rear bumper fascia (6). Refer to Rear Bumper Fascia Replacement .