For 1990-2009 cars

### Removal Procedure

1. Remove the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.
2. Remove the following components from the rear window trim panel (1):

• | The 4 retainers (3)

• | The rear speaker grille (2)

### Installation Procedure

1. Install the rear speaker grille (2) to the rear window trim panel (1). Secure the grille with the 4 retainers (3).
2. Install the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.