For 1990-2009 cars

### Removal Procedure

Important: The ignition switch must be in the OFF position when removing the instrument cluster assembly.

1. Remove the IP cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Remove the 3 screws which secure the instrument cluster assembly.
3. Disconnect the 4 electrical connectors (2) from the cluster assembly (1).
4. Remove the cluster assembly (1) from the instrument panel assembly.

### Installation Procedure

1. Connect the 4 electrical connectors (2) to the instrument cluster assembly (1).
2. Install the cluster assembly to the instrument panel assembly. Secure the assembly with the 3 screws.
3. Install the IP cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .