For 1990-2009 cars

### Removal Procedure

Notice: When removing body panels, apply tape to corners of panel and adjacent surfaces to help prevent paint damage.

1. Remove the following components from the vehicle:

• | The 6 bolts

• | The 8 plastic retainers

• | The front wheelhouse panel liner (1)

2. Remove the front turn signal lamp mounting screw (1).
3. Remove the front turn signal lamp (2) from the vehicle.
4. Disconnect the front turn signal lamp electrical connector.
5. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement in Bumpers.
6. Remove the front fender (1) to rocker panel bolt.
7. Remove the 2 front fender to door jamb (3) bolts.
8. Remove the top 4 front fender (1) bolts.
9. Remove the 2 bolts (2) and 1 nut (3) at the front of the front fender.
10. Remove the front fender (1) from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the front fender (1) to the vehicle. Secure the fender with the 2 bolts (2) and 1 nut (3).

Tighten
Tighten the front fender bolts and nut to 20 N·m (15 lb ft).

2. Install the top 4 front fender (1) bolts.

Tighten
Tighten the top front fender bolts to 20 N·m (15 lb ft).

3. Install the 2 door jamb (3) to front fender bolts.

Tighten
Tighten the door jamb to front fender bolts to 20 N·m (15 lb ft).

4. Install the front fender (1) to rocker panel bolt.

Tighten
Tighten the front fender to rocker panel bolt to 20 N·m (15 lb ft).

5. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement in Bumpers.
6. Connect the front turn signal lamp connector.
7. Install the front turn signal lamp (2) to the vehicle. Secure the lamp with the mounting screw.
8. Install the front wheelhouse panel liner (1) to the vehicle. Secure the panel with the 6 bolts and the 8 plastic retainers.

Tighten
Tighten the wheelhouse panel liner bolts to 10 N·m (89 lb in).