For 1990-2009 cars

### Removal Procedure

1. Tilt the sunroof window into the up position.
2. Remove the following components from the vehicle:

• | The 2 screws (2) which secure each side of the sunroof window

• | The sunroof window (1)

### Installation Procedure

1. Install the sunroof window (1) to the vehicle. Secure each side of the window with the 2 screws (2). Do not tighten fully.
2. Adjust the sunroof window as necessary. Refer to Sunroof Window Height and Opening Fit Adjustment .