For 1990-2009 cars

#### Hesitation, Sag, Stumble

Checks | Action
--- | ---
DEFINITION: The vehicle has a momentary lack of response when pushing down on the accelerator. The condition can occur at any vehicle speed. The condition is usually most severe when trying to make the vehicle move, as from a stop sign. The condition may cause the engine to stall if severe enough.
Preliminary Check |

• | Refer to Powertrain On Board Diagnostic (OBD) System Check .

• | Refer to Symptoms .

Fuel System Checks |

• | Check for a restricted fuel filter or incorrect fuel pressure. Refer to Fuel System Diagnosis .

• | Check the fuel injectors. Perform the Fuel Injector Coil Test Procedure and the Fuel Injector Balance Test Procedure. Refer to Fuel Injector Solenoid Coil Test - Engine Coolant Temperature Between 10-35 Degrees C (50-95 Degrees F) and Fuel Injector Balance Test .

• | Check for water contamination of the fuel.

• | Check the TP sensor for binding or sticking. Voltage should increase at a steady rate as throttle moves toward Wide Open Throttle (WOT).

• | Check the MAP sensor for a quick response and accuracy.

• | Check the Evaporative Emission (EVAP) control system. Refer to Evaporative Emission Control System Diagnosis .

Ignition System Checks |

• | Check for faulty spark plug wires.

• | Check for fouled spark plugs.

Additional Checks |

• | Check the Service Bulletins for any updates.

• | Check the generator output voltage.