For 1990-2009 cars

The services shown in this schedule up to 166 000 km (100,000 miles) should be performed after 166 000 km (100,000 miles) at the same intervals.

### Footnotes

[Dagger] The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance item will not nullify the emission warranty or limit recall liability prior to the completion of the vehicle's useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

# Lubricate the parking brake cable guides, underbody contact points and linkage.

+ A good time to check brakes is during tire rotation. Inspect the complete system. Inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Also inspect drum brake linings for wear and cracks. Inspect other brake parts, including drums, wheel cylinders, calipers parking brake, etc. Check parking brake adjustment. You may need to have your brakes inspected more often if your driving habits or conditions result in frequent braking.

### 5 000 km (3,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 10 000 km (6,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 15 000 km (9,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 20 000 km (12,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 25 000 km (15,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Change automatic transaxle and differential fluid every 25 000 km (15,000 miles) if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service

• | If you do not use your vehicle under any of these conditions, check the fluid.

### 30 000 km (18,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 35 000 km (21,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 40 000 km (24,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 45 000 km (27,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 50 000 km (30,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Replace spark plugs.

• | Replace air cleaner filter (or every 24 months, whichever occurs first).

• | Inspect fuel tank, cap and lines for damage or leaks. Inspect fuel cap gasket for any damage. Replace parts as needed. See footnote [Dagger].

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Drain, flush and refill cooling system (or every 24 months, whichever occurs first). See Explanation of Scheduled Services for what to use. Inspect hoses. Clean radiator, condenser, pressure cap and neck. Pressure test cooling system and pressure cap. See footnote [Dagger].

• | Change manual transaxle fluid every 50 000 km (30,000 miles) only if your vehicle is used to tow a trailer.

• | Change automatic transaxle and differential fluid every 25 000 km (15,000 miles) if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If you do not use your vehicle under any of these conditions, check the fluid.

### 55 000 km (33,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 60 000 km (36,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 65 000 km (39,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 70 000 km (42,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 75 000 km (45,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Change automatic transaxle and differential fluid every 25 000 km (15,000 miles) if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If you do not use your vehicle under any of these conditions, check the fluid.

### 80 000 km (48,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 85 000 km (51,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 90 000 km (54,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 95 000 km (57,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 100 000 km (60,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Inspect engine accessory drive belts (or every 48 months, whichever occurs first).

• | Replace spark plugs.

• | Replace air cleaner filter (or every 24 months, whichever occurs first).

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect for tappet noise and engine vibration. Adjust valve clearance to factory specifications if necessary (or every 48 months, whichever occurs first).

• | Inspect fuel tank, cap, cap gasket and lines for damage or leaks (or every 24 months, whichever occurs first). Replace parts as needed. See footnote [Dagger]

• | Drain, flush and refill cooling system (or every 24 months, whichever occurs first). See Explanation of Scheduled Services for what to use. Inspect hoses. Clean radiator, condenser, pressure cap and neck. Pressure test cooling system and pressure cap. See footnote [Dagger].

• | Change manual transaxle fluid every 50 000 km (30,000 miles) only if your vehicle is used to tow a trailer.

• | Change automatic transaxle and differential fluid every 25 000 km (15,000 miles) if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If you do not use your vehicle under any of these conditions, check the fluid.

### 105 000 km (63,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 110 000 km (66,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 115 000 km (69,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 120 000 km (72,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 125 000 km (75,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Inspect engine accessory drive belts (or 12 months since last inspection).

• | Change automatic transaxle and differential fluid every 25 000 km (15,000 miles) if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If you do not use your vehicle under any of these conditions, check the fluid.

### 130 000 km (78,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 135 000 km (81,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 140 000 km (84,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 145 000 km (87,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 150 000 km (90,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Inspect engine accessory drive belts (or every 12 months since last inspection).

• | Replace spark plugs.

• | Replace air cleaner filter (or every 24 months, whichever occurs first).

• | Inspect fuel tank, cap, cap gasket and lines for damage or leaks (or every 24 months, whichever occurs first). Replace parts as needed. See footnote [Dagger]

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Drain, flush and refill cooling system (or every 24 months, whichever occurs first). See Explanation of Scheduled Services for what to use. Inspect hoses. Clean radiator, condenser, pressure cap and neck. Pressure test cooling system and pressure cap. See footnote [Dagger].

• | Change manual transaxle fluid every 50 000 km (30,000 miles) only if your vehicle is used to tow a trailer.

• | Change automatic transaxle fluid and filter if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

- | In hilly or mountainous terrain.

- | When doing frequent trailer towing.

- | Uses such as found in taxi, police or delivery service.

• | If you do not use your vehicle under any of these conditions, check the fluid.

### 155 000 km (93,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 160 000 km (96,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Inspect the air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

### 165 000 km (99,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).