For 1990-2009 cars

### Removal Procedure

1. Pull the rear compartment lid weatherstrip from the pinch weld flange.
2. Remove the rear compartment lid weatherstrip (2) from the vehicle.

### Installation Procedure

1. Apply a thin bead of weatherstrip adhesive GM P/N 12345096, or equivalent, around the perimeter of the rear compartment lid opening pinch weld flange.
2. Press the rear compartment lid weatherstrip (2) firmly in place to the pinch weld flange.