For 1990-2009 cars

## Air Conditioning Clutch Coil Removal V5 - Direct Mount

#### Tools Required

• | J 41790-A Compressor Holding Fixture

• | J 8433 Compressor Pulley Puller

• | J 8433-3 Forcing Screw

• | J 33025 Clutch Coil Puller Legs

• | J 33023-A Puller Pilot

1. Install the compressor onto the J 41790-A .
2. Install the J 33023-A onto the front head of the compressor.
3. Remove the compressor clutch plate and hub assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal .
4. Remove the compressor rotor and bearing assembly. Refer to Clutch Rotor and/or Bearing Removal .
5. Mark the clutch coil terminal location (2) on the compressor front head.
6. Install the J 33025 onto the J 8433 .
7. Install the J 8433 onto the compressor clutch coil (1) and tighten the puller leg bolts.
8. Tighten the center forcing screw J 8433-3 of the compressor pulley puller J 8433 against the puller pilot to remove the compressor clutch coil from the compressor.