For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Charging System

- Brush Length - Standard

10.5 mm

0.413 in

- Brush Length - Minimum

1.5 mm

0.059 in

- Direction of Rotation

Clockwise (as viewed from pulley side)

- Maximum Generator Output

80 Amps

- Maximum Generator Speed

18,00 RPM

- No-Load Generator Speed

1100 RPM

- Normal Operating Voltage

12 Volts

- Polarity

Negative Ground

- Regulator Voltage

13.5-15.1 volts

- Rotor Slip Ring Diameter - Standard

14.2-14.4 mm

0.559-0.567 in

- Rotor Slip Ring Diameter - Minimum

12.8 mm

0.504 in

- Standard Rotor Resistance at 20°C (68°F)

2.7-3.1ohms

- Temperature Range

30-90°C

-22-194°F

Drive Belt Tension

- Drive Belt Deflection - New

5-7 mm at 10 kg

0.20-0.27 in at 22 lbs

- Drive Belt Deflection - Used

6-8 mm at 10 kg

0.24-0.31 in at 22 lbs

Starting System

- Brush Length - Standard

15.5 mm

0.610 in

- Brush Length - Minimum

10.0 mm

0.394 in

- Brush Spring Tension - Standard

1.8-2.4 kg

4.0-5.3 lbs

- Brush Spring Tension - Minimum

1.2 kg

2.6 lbs

- Commutator Insulation Depth - Standard

0.60 mm

0.024 in

- Commutator Insulation Depth - Minimum

0.20 mm

0.008 in

- Commutator Outside Diameter - Standard

30 mm

1.18 in

- Commutator Outside Diameter - Minimum

29 mm

1.14 in

- Commutator Runout - Standard

0.05 mm

0.002 in

- Direction of Rotation

Clockwise (as viewed from pinion)

- Number of Pinion Teeth

9

- Output

1.4 kwatts

- Rating

30 seconds

- Starter Current Draw, no load

90 Amps at 11.5 Volts

- Starter Current Draw, load, manual transaxle (9.1 N·m/80.5 lb in of torque)

300 Amps at 7.7 Volts

- Starter Current Draw, load, automatic transaxle (10.4 N·m/92 lb in of torque)

300 Amps at 7.7 Volts

- Locked Rotor - Manual Transaxle (18.6 N·m/13.8 lb ft)

780 Amps at 4 Volts

- Locked Rotor - Automatic Transaxle (25.5 N·m/18.8 lb ft)

980 Amps at 4 Volts

- Starter Solenoid Operating Voltage

8 Volts minimum

- Solenoid Contact Plate Wear - Maximum

0.9 mm

0.035 in

- Voltage

12 Volts