For 1990-2009 cars

### Removal Procedure

Caution: When a rear compartment lid hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Remove the rear compartment lid. Refer to Rear Compartment Lid Replacement .
2. Remove the rear window trim panel. Refer to Rear Window Trim Panel Replacement .
3. Remove the rear compartment lid hinge torque rods. Refer to Rear Compartment Lid Hinge Torque Rod Replacement .
4. Remove the following items from the vehicle:

• | The pin (1)

• | The rear compartment lid hinge (2)

### Installation Procedure

1. Install the rear compartment lid hinge (2) to the vehicle. Secure the hinge with the pin (1).
2. Install the rear compartment lid hinge torque rods. Refer to Rear Compartment Lid Hinge Torque Rod Replacement .
3. Install the rear window trim panel. Refer to Rear Window Trim Panel Replacement .
4. Install the rear compartment lid. Refer to Rear Compartment Lid Replacement .