For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the system Descriptions and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Verify that the ride is too hard. Is the ride too hard? | Go to Step 3 | System OK
3 | Inspect the struts for wear or damage. Refer to Suspension Strut and Shock Absorber Testing - On Vehicle . Are any of the struts the worn or damaged? | Go to Step 4 | Go to Step 2
4 | Replace all of the worn or damaged components. Refer to the following procedures:

• | Strut Assembly Replacement in Front Suspension

• | Strut, Strut Component, and Spring Replacement in Front Suspension

• | Strut Assembly Replacement in Rear Suspension

• | Strut Disassemble/Assemble Repair in Rear Suspension

Did you complete the repair?

Go to Step 5

--

5 | Drive the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2