For 1990-2009 cars

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement .
2. Disconnect the power window motor electrical connector (2), if equipped.
3. Remove the following components from the door:

• | The 5 bolts (4)

• | The nut (3)

• | The window regulator (1)

### Installation Procedure

1. Apply a multipurpose grease to all lubrication and sliding points.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the window regulator (1) to the door. Secure the regulator with the 5 bolts (4) and the nut (3).

Tighten
Tighten the regulator bolts and nut to 8 N·m (71 lb in).

3. Connect the power window motor electrical connector (2), if equipped.
4. Install the front door window. Refer to Front Side Door Window Replacement .