For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .
2. Starting at the top, pull downward on the rear side door water deflector (3) in order to remove from the door edges.
3. Unroute the electrical connector (2) and the rear side door inside handle rod (1) from the water deflector (3), while removing the deflector from the vehicle.

### Installation Procedure

1. Route the electrical connector (2) and the rear side door inside handle rod (1) through the rear side door water deflector (3).
2. Install the rear side door water deflector (3) to the door.
3. Install the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .