For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Cut the hog rings around the bottom perimeter of the rear seat cushion (1).
3. Remove the rear seat cushion cover from the cushion.

### Installation Procedure

1. Install the rear seat cushion cover to the seat cushion.
2. Use hog ring pliers (1) to install new hog rings. Ensure that the rear seat cushion cover is secured to the cushion (2).
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .