For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Switch | 40 N·m | 30 lb ft
Bearing Lock Bolts | 11 N·m | 97 lb in
Fifth Gear Lock Nut | 118 N·m | 87 lb ft
Front Bearing Retainer Bolts | 11 N·m | 97 lb in
Lock Ball Assembly Plugs | 13 N·m | 115 lb in
Number 3 Fork Shaft Lock Nut | 16 N·m | 12 lb ft
Oil Receiver Bolts | 11 N·m | 97 lb in
Reverse Idler Shaft Lock Bolt | 39 N·m | 29 lb ft
Reverse Shift Arm Bolts | 17 N·m | 13 lb ft
Ring Bearing Retainer Bolts | 27 N·m | 20 lb ft
Ring Gear Bolts | 77 N·m | 57 lb ft
Select Control Lock Bolt | 29 N·m | 22 lb ft
Shift and Select Lever Assembly Bolts | 20 N·m | 14 lb ft
Shift Shaft Lock Bolts | 16 N·m | 12 lb ft
Transaxle Case Bolts | 29 N·m | 22 lb ft
Transaxle Case Cover Bolts | 18 N·m | 13 lb ft
Vehicle Speed Sensor (VSS) Retaining Bolt | 11 N·m | 97 lb in

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 23 N·m | 17 lb ft
Clutch Line Bracket Bolts | 12 N·m | 106 lb in
Clutch Release Cylinder Bolts | 12 N·m | 106 lb in
Clutch Release Lever Bolt and Nut | 23 N·m | 17 lb ft
Extension Rod Retaining Nut | 40 N·m | 29 lb ft
Flywheel Cover Bolts | 20 N·m | 15 lb ft
Front Transaxle Bolt | 60 N·m | 44 lb ft
Gearshift Control Lever Guide Plate Bolts | 10 N·m | 89 lb in
Gearshift Control Lever Housing Nuts | 6 N·m | 53 lb in
Gearshift Control Lever Housing-to-Guide Plate Nuts | 40 N·m | 29 lb ft
Gearshift Guide Case Bolts | 12 N·m | 106 lb in
Gearshift Interlock Bolt | 28 N·m | 21 lb ft
Gearshift Yoke Bolt | 28 N·m | 21 lb ft
Heat Insulator Bolts and Nut | 20 N·m | 15 lb ft
Hold Down Bracket Bolt and Nut | 12 N·m | 106 lb in
Left Case Cover Bolts | 12 N·m | 106 lb in
Left Transaxle Mount Bracket Bolts | 60 N·m | 44 lb ft
Left Transaxle Mount Bolts | 60 N·m | 44 lb ft
Left Transaxle Mount Retaining Nuts | 60 N·m | 44 lb ft
Left Transaxle Mount Through Bolt | 60 N·m | 44 lb ft
Lower Transmission to Engine Bolts

- #1 Bolts

23 N·m

11 lb ft

- #2 Bolts

46 N·m

34 lb ft

Rear Transaxle Mount Retaining Bolts | 60 N·m | 44 lb ft
Rear 3 Mount Nuts | 57 N·m | 42 lb ft
Rear Transaxle Mount Through Bolt and Nut | 60 N·m | 44 lb ft
Right Case-to-Engine Block Mounting Bolts | 60 N·m | 44 lb ft
Speedometer Driven Gear Case Retaining Bolt | 7 N·m | 62 lb in
Starter Bolts | 39 N·m | 29 lb ft
Starter Motor Retaining Bolts | 28 N·m | 21 lb ft
Transaxle Drain Plug | 21 N·m | 15 lb ft
Transaxle Hanger Bolt | 12 N·m | 106 lb in
Transaxle Oil Level/Filler Plug | 21 N·m | 15 lb ft
Transaxle Side Cover Bolts | 12 N·m | 106 lb in
Transaxle Upper Side Mounting Bolts | 64 N·m | 47 lb ft
Vehicle Speed Sensor Bolt | 6 N·m | 53 lb in