For 1990-2009 cars

## Rear Seat Back Cushion Cover and Pad Replacement Full Width

### Removal Procedure

1. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .
2. Remove the rear seat back cushion. Refer to Rear Seat Back Replacement .
3. Remove the rear seat shoulder belt guides from the rear seat back cushion by gently prying loose.
4. Cut and remove the hog rings around the perimeter of the back of the rear seat back cushion (1).
5. Remove the rear seat back cushion cover from the cushion.

### Installation Procedure

1. Install the rear seat back cushion cover to the seat back cushion.
2. Use hog ring pliers (1) to install new hog rings. Ensure that the rear seat back cushion cover is secured to the cushion (2).
3. Install the rear seat shoulder belt guide to the rear seat back cushion.
4. Install the rear seat back cushion. Refer to Rear Seat Back Replacement .
5. Install the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .

## Rear Seat Back Cushion Cover and Pad Replacement AN2

### Removal Procedure

1. Remove the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .
2. Remove the rear seat back cushion. Refer to Rear Seat Back Replacement .
3. Remove the rear seat shoulder belt guide from the rear seat back cushion by gently prying loose.
4. Cut and remove the hog rings around the perimeter of the back of the rear seat back cushion (1).
5. Remove the rear seat back cushion cover from the cushion.

### Installation Procedure

1. Install the rear seat back cushion cover to the seat back cushion.
2. Use hog ring pliers (1) to install new hog rings. Ensure that the rear seat back cushion cover is secured to the cushion (2).
3. Install the rear seat shoulder belt guide to the rear seat back cushion.
4. Install the rear seat back cushion. Refer to Rear Seat Back Replacement .
5. Install the rear seat head restraint. Refer to Rear Seat Head Restraint Replacement .