For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Wheel Speed Sensor Bolt | 8 N·m | 71 lb in
Ball Stud-to-Control Arm Nuts and Bolt | 142 N·m | 105 lb ft
Ball Stud-to-Steering Knuckle Nut | 124 N·m | 91 lb ft
Brake Caliper-to-Steering Knuckle Set Bolt | 88 N·m | 65 lb ft
Brake Hose Bolt | 29 N·m | 22 lb in
Control Arm-to-Suspension Crossmember Front Bolt | 215 N·m | 158 lb ft
Crossmember Front Outer Bolt | 225 N·m | 167 lb ft
Drive Axle Nut | 225 N·m | 166 lb ft
Dust Cover Bolt | 8.3 N·m | 74 lb in
Engine Crossmember-to-Suspension Crossmember Nut and Bolt | 60 N·m | 45 lb ft
Engine Splash Shield Bolt | 10 N·m | 89 lb in
Front Suspension Crossmember Nut | 57 N·m | 42 lb ft
Front Transaxle Mount Bolt | 64 N·m | 47 lb ft
Left and Right Control Arm Retaining Bracket Inner Bolt | 175 N·m | 129 lb ft
Left and Right Control Arm Retaining Bracket Outer Bolt | 147 N·m | 109 lb ft
Left and Right Control Arm Retaining Bracket Outer Nut | 19 N·m | 14 lb ft
Left and Right Control Arm Retaining Bracket Rear Bolt | 123 N·m | 91 lb ft
Stabilizer Shaft Link Nut | 44 N·m | 33 lb ft
Stabilizer Shaft Mounting Bracket Front Bolt | 225 N·m | 167 lb ft
Stabilizer Shaft Mounting Bracket Nut | 19 N·m | 14 lb ft
Stabilizer Shaft Mounting Bracket Stud | 147 N·m | 109 lb ft
Steering Knuckle-to-Strut Assembly Nut | 274 N·m | 203 lb ft
Strut Assembly Mounting Nut | 39 N·m | 29 lb ft
Strut Rod Piston Nut | 47 N·m | 34 lb ft
Suspension Support Brace Nut | 69 N·m | 51 lb ft
Tie Rod End Nut | 49 N·m | 36 lb ft