For 1990-2009 cars

Do not use the following methods for wheel repair:

• | Welding

• | Heating

• | Peening

Replace the wheels if any of the following conditions exist:

• | The wheels are dented

• | The wheels have excessive lateral runout

• | The wheels have excessive radial runout

• | Air leaks through the welds

• | The wheels have elongated bolt holes

• | The wheel nuts do not remain securely attached

• | The wheel nuts are heavily rusted

Do not repair a leaky wheel or tire with an inner tube.