For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner (ACL) Mounting Bolts | 7 N·m | 62 lb in
Camshaft Bearing Cap Bolts | 19 N·m | 14 lb ft
Camshaft Sensor Bolt | 15 N·m | 11 lb ft
Camshaft Timing Sprocket Bolts | 55 N·m | 40 lb ft
Connecting Rod Bearing Cap Bolts

- First Pass

30 N·m

22 lb ft

- Second Pass

90°

90°

Coolant Bypass Pipe to Cylinder Head Bolt | 15 N·m | 11 lb ft
Crankshaft Position Sensor Bolt | 9 N·m | 80 lb in
Crankshaft Pulley Bolt | 118 N·m | 87 lb ft
Cylinder Head Cover Bolts and Nuts | 10 N·m | 7 lb ft
Cylinder Head Bolts

- First Pass

35 N·m

26 lb ft

- Second Pass

180°

180°

Drive Belt Tensioner Bolt | 100 N·m | 74 lb ft
Drive Belt Tensioner Nut | 29 N·m | 21 lb ft
Engine Coolant Drain Union | 25 N·m | 18 lb ft
Engine Crossmember To Body Bolts | 39 N·m | 29 lb ft
Engine Mount (LH Side) Bolts | 80 N·m | 60 lb ft
Engine Mount Bolts (RH Side) | 52 N·m | 38 lb ft
Engine Mount Insulator Bolts (RH Side) | 52 N·m | 38 lb ft
Engine Oil Drain Plug | 35 N·m | 26 lb ft
Engine Oil Pan Nuts and Bolts | 9 N·m | 80 lb in
Exhaust Bracket-to-Exhaust Manifold Bolt | 35 N·m | 26 lb ft
Exhaust Manifold Flange Bolts | 62 N·m | 46 lb ft
Exhaust Manifold Heat Shield Bolts | 20 N·m | 15 lb ft
Exhaust Manifold-to-Bracket Bolts | 50 N·m | 37 lb ft
Exhaust Manifold-to-Cylinder Head Bolts | 50 N·m | 37 lb ft
Exhaust Pipe-to-Three Way Catalytic Converter (TWC) Clamp Bolt | 43 N·m | 32 lb ft
Front Engine Mount To Engine Mount Crossmember | 52 N·m | 38 lb ft
Fuel Injector Harness Bolts | 12 N·m | 106 lb in
Flywheel Retaining Bolts

- First Pass

49 N·m

36 lb ft

- Second Pass

90°

90°

Fuel Rail to Cylinder Head Bolts | 14 N·m | 10 lb ft
Generator Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Heated Oxygen (HO2S1) Sensor | 44 N·m | 32 lb ft
Ignition Coil Bracket Bolts | 14 N·m | 10 lb ft
Intake Manifold Nuts and Bolts

- Upper Bolts

34 N·m

25 lb ft

- Lower Bolt

46 N·m

34 lb ft

Intake Manifold Support Bracket Bolts | 50 N·m | 37 lb ft
Knock Sensor Bolt | 39 N·m | 29 lb ft
Lower Crankcase Bolts | 18 N·m | 13 lb ft
Main Bearing Cap Bolts

- First Pass

22 N·m

16 lb ft

- Second Pass

44 N·m

32 lb ft

- Third Pass

45°

45°

- Third Pass (Final Torque)

45°

45°

Oil Control Valve Filter | 9 N·m | 80 lb in
Oil Control Valve Housing To Cylinder Head Bolts | 9 N·m | 80 lb in
Oil Filter Adapter | 30 N·m | 17 lb ft
Oil Level Indicator Guide Tube Bolt | 24 N·m | 18 lb ft
Oil Pan Baffle | 9 N·m | 80 lb in
Oil Pressure Switch | 13 N·m | 9 lb ft
Oil Pump Bolts | 11 N·m | 97 lb in
Oil Pump Strainer Bolt | 9 N·m | 80 lb in
Oil Pump Strainer Bracket Bolt | 11 N·m | 97 lb in
Power Steering Pump Bolts | 36 N·m | 27 lb ft
Rear Engine Mount Bracket To Suspension Crossmember | 87 N·m | 64 lb ft
Spark Plugs | 28 N·m | 21 lb ft
Starter Bolts | 30 N·m | 22 lb ft
Suspension Crossmember To Body Bolts
Crossmember Front Bolts | 157 N·m | 116 lb ft
Crossmember Rear Bolts | 113 N·m | 83 lb ft
Throttle Body Nuts and Bolts | 23 N·m | 17 lb ft
Timing Chain Cover Nut and Bolts (10 mm head) | 10 N·m | 89 lb in
Timing Chain Cover Nut and Bolts (12 mm head) | 18 N·m | 14 lb ft
Timing Chain Cover Stud Nut | 9.3 N·m | 80 lb in
Timing Chain Dampener Bolt | 21 N·m | 15 lb ft
Timing Chain Shoe Bolts | 10 N·m | 89 lb in
Timing Chain Tensioner Bolts | 21 N·m | 15 lb ft
Timing Controller Assembly | 55 N·m | 40 lb ft
Torque Converter Bolts | 35 N·m | 26 lb ft
Transmission to Engine Mounting Bolts | 64 N·m | 47 lb ft
Ventilation Pipe To Cylinder Head Cover | 10 N·m | 7 lb ft
Ventilation Pipe To Intake Manifold | 25 N·m | 18 lb ft
Water Bypass Pipe To Cylinder Block

- Bolt

8.5 N·m

75 lb in

- Nut

10 N·m

7 lb ft

Water Bypass Pipe To Cylinder Head | 9 N·m | 80 lb in
Water Jacket Plug | 25 N·m | 18 lb ft
Water Pump Bolts | 12 N·m | 106 lb in
Windshield Washer Reservoir Bolt | 10 N·m | 89 lb in