For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Radio/Audio system check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 | Does the radio briefly display CLN TAPE when a tape is inserted? | -- | Go to Step 5 | Go to Step 3
3 | Using the test tape from the J 39916-A , perform the motor speed test, following the instructions in the kit. Is the tape speed within the allowable limits? | -- | Go to Step 4 | Go to Step 6
4 | Play a known good tape in the player and determine if the output is garbled or distorted. The speaker test tones included in the J 39916-A test tape may be used to help identify a problem. Is the audio quality OK? | -- | Go to Step 7 | Go to Step 5
5 |

1. Clean the tape heads using the tape cleaner included in the J 39916-A .
2. After cleaning, reset the tape clean meter (CLN) display if present, by pressing the cassette eject control for 5 seconds.
3. Play a known good tape.

Is the audio quality OK?

--

Go to Step 7

Go to Step 6

6 | Replace the radio. Refer to Radio Replacement . Is the repair complete? | -- | Go to Step 7 | --
7 | Repeat the system check. Refer to Radio/Audio System Check . Is the system check complete? | -- | System OK | --