For 1990-2009 cars

### Circuit Description

The pump motor relay is part of the Electronic Brake Control Module (EBCM). The EBCM turns ON and OFF the pump motor relay as deemed necessary to activate the pump motor.

### Conditions for Running the DTC

DTC C0110 can be set anytime the pump motor is actuated.

### Conditions for Setting the DTC

The EBCM detects a stuck pump motor.

### Action Taken When the DTC Sets

• | The ABS is disabled.

• | The ABS warning indicator turns ON.

### Conditions for Clearing the DTC

• | The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

• | After the DTC is cleared, the ABS indicator will remain ON until the vehicle is road tested to verify the repair. Once the vehicle has been driven at a speed above 16 km/h (10 mph) for 20 seconds with no malfunctions present, the EBCM will turn OFF the ABS indicator.

### Diagnostic Aids

Thoroughly inspect the wiring and the connectors. An incomplete inspection of the wiring and the connectors may result in a misdiagnosis, causing a part replacement with the reappearance of the malfunction.

The following are possible causes of the malfunction:

• | An open, high resistance, or a short to ground in the battery positive voltage circuits

• | An open or high resistance in the motor ground circuit

• | An internal EBCM malfunction

If an intermittent malfunction exists, refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

### Test Description

The number below refers to the step number on the Diagnostic Table.

1. This step determines if the DTC is current.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Antilock Brake System Schematics
1 | Did you perform A Diagnostic System Check - ABS? | Go to Step 2 | Go to Diagnostic System Check - ABS
2 | Is DTC C0114 also set? | Go to DTC C0114 | Go to Step 3
3 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. Use the scan tool in order to clear the DTCs.
4. Using the scan tool, cycle the pump motor in the Special Functions menu.
5. Read the DTCs.

Does the DTC reset?

Go to Step 4

Go to Diagnostic Aids

4 |

1. Test the Battery Positive Voltage circuits for an open, high resistance, or a short to ground. Refer to Circuit Testing and Wiring Repairs in Wiring Systems.
2. Test the Motor Ground circuit for an open or high resistance. Refer to Circuit Testing and Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

Go to Step 6

Go to Step 5

5 | Replace the Brake Pressure Modulator Valve (BPMV). Refer to Brake Pressure Modulator Valve Assembly Replacement . Did you complete the replacement? | Go to Step 6 | --
6 |

1. Use the scan tool in order to clear the DTCs.
2. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC reset?

Go to Step 2

System OK