For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Instrument Cluster Schematics
1 | Did you review the Instrument Panel, Gages and Console Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Instrument Panel, Gages and Console
2 | Verify that the instrument cluster gages are inoperative. Does the system operate normally? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 |

1. Disconnect the instrument cluster connector C1.
2. Test for an open condition between cavity 14 and a good ground.

Does an open condition exist?

Go to Step 4

Go to Step 5

4 | Repair the open in the BLK/WHT wire between the instrument cluster and the junction block C4 cavity 1. Did you complete the repair? | Go to Step 9 | --
5 |

1. Disconnect the instrument cluster connector C3.
2. Test for a open condition between cavity 2 and G103.

Does an open condition exist?

Go to Step 6

Go to Step 7

6 | Repair the short in the BLK/YEL wire between the instrument cluster and G103. Did you complete the repair? | Go to Step 9 | --
7 | Inspect the instrument cluster for any damage to the cluster or printed circuit. Is there any damage to the instrument cluster or printed circuit? | Go to Step 8 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
8 | Repair or replace the instrument cluster or printed circuit. Did you complete the repair? | Go to Step 9 | --
9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3