For 1990-2009 cars

### Removal Procedure

1. Remove the manual transaxle control lever knob (1) from the manual transaxle control lever by turning in a counterclockwise direction.
2. Remove the manual transaxle control lever boot (2) from the control lever by pulling up to disengage the boot from the manual transaxle control lever boot retainer.
3. Remove the boot retainer (3) from the front floor consoles (2) by releasing the 2 retaining tabs.

### Installation Procedure

1. Install the manual transaxle control lever boot (1) to the manual transaxle lever boot retainer (2).
2. Install the boot and retainer assembly (2) to the front floor consoles. Ensure that the retaining tabs are fully engaged.
3. Install the manual transaxle control lever knob (1) to the manual transaxle control lever by turning in a clockwise direction.