For 1990-2009 cars

#### Tools Required

• | J 22912-B Bearing Puller

• | J 35565 Intermediate Shaft Bearing Installer

• | J 35378 Puller Pilot

### Removal Procedure

Use J 22912-B and J 35378 in order to remove the intermediate shaft rear bearing.

### Installation Procedure

1. Use J 35565 in order to install the intermediate shaft rear bearing.
2. Verify that the distance from the gear flange end to the intermediate shaft is approximately 115.8 mm (4.559 in).