For 1990-2009 cars

### Removal Procedure

1. Gently pry loose the high mounted stoplamp and cover assembly (2).
2. Disconnect the high mounted stoplamp electrical connector.
3. Remove the stoplamp (1) from the cover (3).
4. Remove the lamp socket (2) from the stoplamp (1), if necessary.
5. Remove the bulb from the lamp socket (2), if necessary.

### Installation Procedure

1. Install the bulb to the lamp socket (2), if removed.
2. Install the lamp socket (2) to the stoplamp (1), if removed.
3. Install the stoplamp (1) to the cover (3).
4. Connect the high mounted stoplamp electrical connector.
5. Install the high mounted stoplamp and cover assembly (2) to the vehicle.