For 1990-2009 cars

### Removal Procedure

1. Remove the speedometer (2). Refer to Speedometer Replacement .
2. Remove the engine tachometer (1), if equipped. Refer to Tachometer Replacement .
3. Remove the fuel gauge (3), if equipped. Refer to Fuel Gage Replacement .
4. Remove the engine coolant temperature gauge (4), if equipped. Refer to Engine Coolant Temperature Gage Replacement .
5. Remove the fuel and temperature gauge (1), if equipped. Refer to Fuel/Temperature Gage Replacement .
6. Remove all of the instrument cluster bulb sockets from the cluster case.
7. Remove the bulbs from the sockets, as necessary.
8. Remove the following relays from the cluster case:

• | Electronic Brake Control Indicator Lamp

• | Instrument Cluster Bulb Check

9. Remove the printed instrument cluster circuit from the instrument cluster case.

### Installation Procedure

1. Install the printed instrument cluster circuit to the instrument cluster case.
2. Install the relays to the cluster case.
3. Install the bulbs to the sockets, if removed.
4. Install all of the instrument cluster bulb sockets to the cluster case.
5. Install the fuel and temperature gauge (1), if equipped. Refer to Fuel/Temperature Gage Replacement .
6. Install the engine coolant temperature gauge (4), if equipped. Refer to Engine Coolant Temperature Gage Replacement .
7. Install the fuel gauge (3), if equipped. Refer to Fuel Gage Replacement .
8. Install the engine tachometer (1), if equipped. Refer to Tachometer Replacement .
9. Install the speedometer (2). Refer to Speedometer Replacement .