For 1990-2009 cars

### Removal Procedure

1. Disconnect the power steering pressure (PSP) switch (1) electrical connector.
2. Remove the PSP switch (1) from the high pressure power steering line above the power steering pump (2).

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the PSP switch (1) into the high pressure power steering line above the power steering pump (2).

Tighten
Tighten the PSP switch to 21 N·m (15 lb ft).

2. Connect the PSP switch electrical connector.