For 1990-2009 cars

Problem | Action
--- | ---
The springs are broken or sagging. | Inspect and repair as necessary. Refer to Strut, Strut Component, and Spring Replacement in Front Suspension or Strut Disassemble/Assemble Repair in Rear Suspension.
The stabilizer shaft is loose or disconnected. | Inspect the following items for damage. Replace as necessary.

• | The stabilizer shaft

• | The stabilizer shaft links

• | The stabilizer shaft brackets

• | The stabilizer shaft insulators

Refer to one of the following procedures:

• | Suspension Component Inspection in Front Suspension

• | Suspension Component Inspection in Rear Suspension

• | Stabilizer Shaft Replacement in Front Suspension

• | Stabilizer Shaft Replacement in Rear Suspension

The vehicle is overloaded. | Reduce the vehicle load. Refer to the Tire Placard on the I/P compartment door.
The tire pressure(s) is incorrect. | Inflate the tire(s) to proper specifications. Refer to the Tire Placard on the I/P compartment door.