For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the IP drivers knee bolster reinforcement. Refer to Knee Bolster Replacement .
3. Remove the screw (2) from Junction Block #2 (1) and position the junction block in order to gain access to the multifunction alarm module.
4. Disconnect the 2 multifunction alarm module electrical connectors.
5. Disconnect the multifunction alarm module (1) from the rear of Junction Block #2 (2).

### Installation Procedure

1. Install the multifunction alarm module (1) to the rear of Junction Block #2 (2).
2. Connect the 2 multifunction alarm module electrical connectors.
3. Reposition Junction Block #2 (1) back into position. Secure the junction block with the screw (2).
4. Install the IP drivers knee bolster reinforcement. Refer to Knee Bolster Replacement .
5. Connect the negative battery cable.