For 1990-2009 cars

### Removal Procedure

1. Push in the tab (3) on the head restraint guide.
2. Lift and remove the head restraint (1).
3. Gently pry loose the head restraint guide (1). Remove the guides from the seat back cushion (2), if necessary.

### Installation Procedure

1. Install the head rest guides to the seat back cushion (2), if removed.
2. Align the head restraint posts into the guides.
3. Push in the tab (3) on the head restraint guide in order to install the head restraint (1). Ensure that the retainer lock engages.