For 1990-2009 cars

Table 1: | General Specifications
Table 2: | Extension Housing Shim Calculation Table - Procedure A
Table 3: | Extension Housing Shim Calculation Table - Procedure B

#### General Specifications

Application | Specification
--- | ---
Metric | English
Differential Bearing Preload | 0.1-0.15 mm | 0.004-0.006 in
Differential Carrier Rotating Torque | 1.5 N·m | 13 lb in
Drive and Drivenshafts Gears Backlash | 0.2-0.3 mm | 0.0078-0.0118 in
Drivenshaft Rotating Torque | 1.5 N·m | 13 lb in
Driveshaft Bearing Preload | 0.15 mm | 0.006 in
Driveshaft Rotating Torque | 1.5 N·m | 13 lb in
Extension Housing Gear Oil Fill Quantity | 290 ml | 9.80 oz
Gear Ratio Front-to-Rear | 1.013:1
Idler Gear Bearing Preload | 1.02-1.78 mm | 0.004-0.007 in

#### Extension Housing Shim Calculation Table - Procedure A

Calculation | Comment | Metric | English
--- | --- | --- | ---
| Actual Measurements |
A | A = Nominal or "Given" Value | 57 mm | 2.24 in
-B | Subtract B = Pinion Thickness |  |
+C | Add C = Pinion Installed Height |  |
-D | Subtract D = Driveshaft Housing Calculated Value |  |
+/- | Add or Subtract the Plus, Minus, or Zero Value Etched on the End of the Driveshaft |  |
| = Extension Housing Shim Thickness |  |

#### Extension Housing Shim Calculation Table - Procedure B

Calculation | Comment | Metric | English
--- | --- | --- | ---
| Actual Measurements |
C | Pinion Installed Height |  |
+E | Add E = Measured Value on the End of the Drivenshaft |  |
F | C plus E equals F, the Pinion Calculated Height |  |
D | Driveshaft Housing Calculated Value |  |
-F | D minus F equals the Extension Housing Shim Thickness |  |
| = Extension Housing Shim Thickness |  |