For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the knob.
3. Remove the boot.
4. Remove the front and rear console.
5. Remove the shift cable end clips.
6. Remove the retainer clips and the shift cables.
7. Remove the shift control.

### Installation Procedure

1. Install the shift control.
2. Install the shift cable and the retainer clips.
3. Install the shift cable end clips.
4. Install the front and rear console.
5. Install the boot.
6. Install the knob.