For 1990-2009 cars

### Removal Procedure

Important: It is not necessary to remove the steering wheel in order to access the screws that retain the steering column lower trim cover. Rotate the steering wheel in order to access the 2 trim cover screws.

1. Remove the 2 lower trim cover screws (2) that are located behind the steering wheel (1).
2. Remove the screw from the bottom of the lower trim cover.
3. Remove the lower trim cover (6).
4. Remove the screw (3) from the upper trim cover.
5. Remove the steering column upper trim cover (2).

### Installation Procedure

1. Install the upper trim cover (2) to the steering column.
2. Install the screw (3) to the upper trim cover.
3. Install the lower trim cover (6) to the steering column.
4. Install the screw to the bottom of the lower trim cover.
5. Install the 2 lower trim cover screws (2) to the lower trim cover.