For 1990-2009 cars

### Removal Procedure

1. Lower the window.
2. Remove the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the water deflector (3) from the rear door.
4. Remove the window run channel weatherstrip (2) from the guide channel.

### Installation Procedure

1. Partially raise the window.
2. Install the window run channel weatherstrip (2) to the guide channel.
3. Install the water deflector (3) to the rear door.
4. Install the rear side door trim. Refer to Rear Side Door Trim Panel Replacement .