For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster retainer. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .

Important: Do not remove the needle from the fuel gauge. There is no detent or flat spot on the shaft in order to indicate the correct placement.

2. Remove the 3 screws (1) which secure the fuel gauge to the instrument cluster case.
3. Remove the fuel gauge (3) from the instrument cluster case.

### Installation Procedure

1. Install the fuel gauge (3) to the instrument cluster case.
2. Secure the fuel gauge with the 3 screws (1).
3. Install the instrument cluster retainer. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .