For 1990-2009 cars

### Circuit Description

This DTC identifies a malfunction within the EBCM.

### Conditions for Running the DTC

The ignition switch is in the ON position.

### Conditions for Setting the DTC

An internal EBCM malfunction exists.

### Action Taken When the DTC Sets

The following actions occur:

• | The ABS is disabled.

• | The ABS warning indicator turns ON.

### Conditions for Clearing the DTC

The condition responsible for setting the DTC no longer exists and the scan tool Clear DTCs function is used.

### Diagnostic Aids

The EBCM is an integral part of the Brake Pressure Modulator Valve (BPMV) and cannot be serviced separately.

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform A Diagnostic System Check - ABS? | Go to Step 2 | Go to Diagnostic System Check - ABS
2 | Replace the Brake Pressure Modulator Valve (BPMV). Refer to Brake Pressure Modulator Valve Assembly Replacement . Did you complete the replacement? | System OK | --