For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the front park/turn signal lamp screw (1).
3. Pull the front park/turn signal lamp (2) forward.
4. Remove the front park/turn signal lamp socket from the lamp lens.
5. Remove the bulb from the socket.

### Installation Procedure

1. Install the bulb to the socket.
2. Install the socket to the front park/turn signal lamp lens (2).
3. Install the front park/turn signal lamp into position. Secure the lamp with the one screw (1).
4. Close the hood.