For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Exterior Lights Schematics
1 | Did you review the Lighting System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Lighting Systems
2 | Verify that the hazard lamps are always on. Does the system operate normally? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 | Replace the hazard switch. Refer to Hazard Flasher Switch Replacement . Is the replacement complete? | Go to Step 4 | --
4 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3