For 1990-2009 cars

## Door Lock and Side Window Switch Replacement Left Front Door

### Removal Procedure

1. Using a taped flat bladed tool, gently pry the front side door accessory switch mounting plate (1) from the front side door trim (2).
2. Disconnect the front side door window/lock switch electrical connector (2).
3. Remove the following components from the front side door window/lock switch (3):

• | The 3 screws (1)

• | The front side door accessory switch mounting plate (2)

### Installation Procedure

1. Install the front side door window/lock switch (3) to the front side door accessory switch mounting plate (2). Secure the switch with the 3 screws (1).
2. Connect the front side door window/lock switch electrical connector (2).
3. Install the front side door accessory switch mounting plate (2) to the front side door trim (1).