For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioner (A/C) Compressor Bracket Mounting Bolts | 55 N·m | 40 lb ft
Air Conditioner (A/C) Compressor Mounting Bolts | 23 N·m | 17 lb ft
Camshaft Bearing Cap Bolts | 12 N·m | 106 lb in
Camshaft Position Sensor Bolt | 15 N·m | 11 lb ft
Camshaft Timing Sprocket Bolts | 80 N·m | 58 lb ft
Connecting Rod Bearing Cap Nuts | 45 N·m | 33 lb ft
Crankshaft Position Sensor Bolt | 6 N·m | 53 lb in
Crankshaft Pulley Bolt | 150 N·m | 109 lb ft
Cylinder Head Bolts

- First Pass

53 N·m

39 lb ft

- Second Pass

84 N·m

61 lb ft

- Third Pass

Loosen to 0

- Fourth Pass

53 N·m

39 lb ft

- Fifth Pass

84 N·m

61 lb ft

- Sixth Pass - Final Torque

105 N·m

76 lb ft

Cylinder Head Cover Bolts | 10.5 N·m | 93 lb in
Cylinder Head M 6 Bolt | 11 N·m | 97 lb in
Drive Belt Tensioner Bolts

- Accessory Drive Belt Tensioner Bolts

25 N·m

19 lb ft

Engine Cooling Fan Nuts | 25 N·m | 18 lb ft
Engine Ground Wire Bolts | 15 N·m | 11 lb ft
Engine Mount Nuts | 50 N·m | 37 lb ft
Engine Oil Drain Plug | 35 N·m | 26 lb ft
Engine Oil Pan Nuts and Bolts | 11 N·m | 97 lb in
Exhaust Manifold Heat Shield Bolts | 10 N·m | 89 lb in
Exhaust Manifold-to-Bracket Bolts | 50 N·m | 37 lb ft
Exhaust Manifold-to-Cylinder Head Nuts | 30 N·m | 22 lb ft
Flywheel Retaining Bolts

- Automatic Transmission

70 N·m

51 lb ft

Fuel Rail Banjo Fitting | 30 N·m | 22 lb ft
Generator Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Generator Terminal Nut | 8 N·m | 71 lb in
Heated Oxygen (HO2S1 and HO2S2) Sensor | 45 N·m | 33 lb ft
Ignition Coil Bolts | 10 N·m | 89 lb in
Intake Manifold Bolts and Nuts | 23 N·m | 17 lb ft
Lower Crankcase Bolts

- First Pass

19 N·m

14 lb ft

- Second Pass - Final Torque

27 N·m

20 lb ft

Main Bearing Cap Bolts

- First Pass

42 N·m

31 lb ft

- Second Pass - Final Torque

58 N·m

42 lb ft

Negative Battery Cable | 15 N·m | 11 lb ft
Oil Pressure Switch | 14 N·m | 11 lb ft
Oil Pump Bolts | 27 N·m | 20 lb ft
Oil Pump Case Bolts | 12 N·m | 106 lb in
Oil Pump Strainer Bolts | 11 N·m | 97 lb in
Power Steering Pump Bolts | 25 N·m | 19 lb ft
Spark Plugs | 25 N·m | 18 lb ft
Starter Bolts | 11 N·m | 97 lb in
Strut Tower Brace | 50 N·m | 37 lb ft
Throttle Body Bolts and Nuts | 12 N·m | 106 lb in
Timing Chain Cover Nut and Bolts | 11 N·m | 97 lb in
Timing Chain Guide Bolts - Primary | 9 N·m | 79 lb in
Timing Chain Tensioner Bolts - Left Camshaft | 12 N·m | 106 lb in
Timing Chain Tensioner Bolts - Right Camshaft | 11 N·m | 97 lb in
Timing Chain Tensioner Bolts - Primary | 11 N·m | 97 lb in
Timing Chain Tensioner Nuts - Left Camshaft | 45 N·m | 33 lb ft
Timing Chain Tensioner Shoe Nut - Primary | 27 N·m | 20 lb ft
Torque Converter Bolts | 65 N·m | 47 lb ft
Transmission to Engine Mounting Bolts | 80 N·m | 58 lb ft
Water Pump Bolts | 27 N·m | 20 lb ft