For 1990-2009 cars

1. Visually inspect the adjuster spring (18) for the following:

• | Excessive corrosion

• | Excessive stretching

• | Broken hook ends

• | Twisting or binding

• | Missing

2. Visually inspect the adjuster actuator lever (2) for the following conditions:

• | Bent

• | Broken

• | Missing

• | Broken spring attachment tab

3. Replace the drum brake adjusting hardware if necessary. Refer to Drum Brake Adjusting Hardware Replacement .