For 1990-2009 cars

#### Tools Required

• | J 39500-B A/C Refrigerant Recovery, Recycling and Recharging (ACR4) System

• | J 41810 Pureguard 2

• | J 41810-100A High Intensity Black Light

Caution: Avoid breathing the A/C Refrigerant 134a (R-134a) and the lubricant vapor or the mist. Exposure may irritate the eyes, nose, and throat. Work in a well ventilated area. In order to remove R-134a from the A/C system, use service equipment that is certified to meet the requirements of SAE J 2210 (R-134a recycling equipment). If an accidental system discharge occurs, ventilate the work area before continuing service. Additional health and safety information may be obtained from the refrigerant and lubricant manufacturers.

Caution: For personal protection, goggles and lint-free gloves should be worn and a clean cloth wrapped around fittings, valves, and connections when doing work that includes opening the refrigerant system. If refrigerant comes in contact with any part of the body severe frostbite and personal injury can result. The exposed area should be flushed immediately with cold water and prompt medical help should be obtained.

Notice: R-134a is the only approved refrigerant for use in this vehicle. The use of any other refrigerant may result in poor system performance or component failure.

Notice: To avoid system damage use only R-134a dedicated tools when servicing the A/C system.

Notice: Use only Polyalkylene Glycol Synthetic Refrigerant Oil (PAG) for internal circulation through the R-134a A/C system and only 525 viscosity mineral oil on fitting threads and O-rings. If lubricants other than those specified are used, compressor failure and/or fitting seizure may result.

Notice: R-12 refrigerant and R-134a refrigerant must never be mixed, even in the smallest of amounts, as they are incompatible with each other. If the refrigerants are mixed, compressor failure is likely to occur. Refer to the manufacturer instructions included with the service equipment before servicing.

The J 39500-B removes the Refrigerant-134a from the vehicle's A/C system. The recovery procedure uses one filtering cycle. The evacuation procedure uses an automatic multiple pass filtering cycle. These filtering cycles ensure a constant supply of clean, dry refrigerant for A/C system charging.

The Initial Set-Up Instruction Manual, provided with the J 39500-B , contains specific procedures for proper recovery, evacuation and recharging.

For ACR4 technical assistance in the U.S., call 1-800-345-2233.