For 1990-2009 cars

## Inflatable Restraint Front End Discriminating Sensor Replacement LH

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the LH front engine splash shield. Refer to Engine Splash Shield Replacement .
3. Remove the electrical connector (1).
4. Remove the fasteners (3).
5. Remove the front end discriminating sensor (2).

### Installation Procedure

1. Enable the SIR system. Refer to Enabling the SIR System .
2. Install the front end discriminating sensor (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the fasteners (3).

Tighten
Tighten the fasteners to 20 N·m (14 lb ft).

4. Install the electrical connector (1).
5. Install the LH front engine splash shield. Refer to Engine Splash Shield Replacement .

## Inflatable Restraint Front End Discriminating Sensor Replacement RH

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Remove the RH front turn signal lamp. Refer to Front Turn Signal Lamp Removal Procedure.
3. Remove the RH headlamp. Refer to Headlamp Assembly Replacement.
4. Remove the electrical connector (1).
5. Remove the fasteners (2).
6. Remove the front end discriminating sensor (3).

### Installation Procedure

1. Enable the SIR system. Refer to Enabling the SIR System .
2. Install the front end discriminating sensor (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the fasteners (2).

Tighten
Tighten the fasteners to 20 N·m (14 lb ft).

4. Install the electrical connector (1).
5. Install the RH headlamp. Refer to Headlamp Assembly Replacement.
6. Install the RH front turn signal lamp. Refer to Front Turn Signal Lamp Installation Procedure.